{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["XSA-Calc"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"XSA-Calc","index":0,"n_rows":56,"n_cols":18,"rows_kept":56,"cut":false,"hidden":false,"merged":[[7,7,7,9],[2,7,6,9],[53,7,53,9],[49,2,49,7],[50,2,50,7],[51,2,51,7],[52,2,52,7],[12,3,12,6],[13,3,13,6],[14,3,14,6],[15,3,15,6],[54,7,54,9],[55,7,55,9],[53,1,55,2],[53,3,53,6],[54,3,54,6],[55,3,55,6]]}
[]
[]
[null,"Rev","Description","By","Chkd","Appd","Date"]
[null,0,"First Issue","ABC",null,null,"2012-11-10"]
[null,1]
[null,2]
[null,3]
[null,4,null,null,null,null,null,"Process Calculation Sheet"]
[null,"V-12A"]
[]
[null,null,"XSA-Calc","Vessel Cross Sectional Area Calculator"]
[]
[null,null,"Project Name","Test Project"]
[null,null,"Customer","ABC Inc"]
[null,null,"Vessel Name","Surge Drum"]
[null,null,"Tag No","V-001"]
[]
[]
[null,null,"Case",null,"A","B","C",null,null,null,null,null,null,null,null,{"$f":"E19","v":"A"},{"$f":"F19","v":"B"},{"$f":"G19","v":"C"}]
[null,null,"Vessel Internal Diameter, D","mm",1500,2000,2000,null,null,null,null,null,null,null,null,{"$f":"E20/1000","v":1.5},2,2]
[null,null,"Height of Fluid, h","mm",225,1000,1500,null,null,null,null,null,null,null,null,0.22500000000000001,1,1.5]
[]
[null,null,"% of Diameter to Level H","%",{"$f":"E21/E20","v":0.15},{"$f":"F21/F20","v":0.5},{"$f":"G21/G20","v":0.75},null,null,null,null,null,null,null,null,{"$f":"E23/1000","v":1.4999999999999999E-4},5.0000000000000001E-4,7.5000000000000002E-4]
[null,null,"% of Total Area to Level H","%",{"$f":"P33/P41","v":9.40602021870936E-2},{"$f":"Q33/Q41","v":0.5},{"$f":"R33/R41","v":0.80449889052211476},null,null,null,null,null,null,null,null,9.4060202187093596E-5,5.0000000000000001E-4,8.0449889052211477E-4]
[]
[null,null,"Area below Level h (Liquid)","m2",{"$f":"P33","v":0.16621809760470591},{"$f":"Q33","v":1.5707963267948966},{"$f":"R33","v":2.5274078042854149},null,null,null,null,null,null,null,"R = D/2",{"$f":"P20/2","v":0.75},{"$f":"Q20/2","v":1},{"$f":"R20/2","v":1}]
[null,null,"Area above Level h (Gas)","m2",{"$f":"E28-E26","v":1.6009277700395528},{"$f":"F28-F26","v":1.5707963267948966},{"$f":"G28-G26","v":0.61418484930437822}]
[null,null,"100% Sectional Area, π*r2","m2",{"$f":"P41","v":1.7671458676442586},{"$f":"Q41","v":3.1415926535897931},{"$f":"R41","v":3.1415926535897931},null,null,null,null,null,null,null,"R^2",{"$f":"P26^2","v":0.5625},{"$f":"Q26^2","v":1},{"$f":"R26^2","v":1}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"R-h",{"$f":"P26-P21","v":0.52500000000000002},{"$f":"Q26-Q21","v":0},{"$f":"R26-R21","v":-0.5}]
[null,null,"Width at Surface, W","mm",{"$f":"P35*1000","v":1071.2142642814276},{"$f":"Q35*1000","v":2000},{"$f":"R35*1000","v":1732.0508075688772},null,null,null,null,null,null,null,"(R-h)^2",{"$f":"P29^2","v":0.27562500000000001},{"$f":"Q29^2","v":0},{"$f":"R29^2","v":0.25}]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"To H","To H","To H"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Af = R2 * cos-1((R-h)/R) - (R-h)*sqrt(2*R*h-h2)",{"$f":"P26^2*(ACOS((P26-P21)/P26))-((P26-P21)*SQRT(2*P26*P21-P21^2))","v":0.16621809760470591},{"$f":"Q26^2*(ACOS((Q26-Q21)/Q26))-((Q26-Q21)*SQRT(2*Q26*Q21-Q21^2))","v":1.5707963267948966},{"$f":"R26^2*(ACOS((R26-R21)/R26))-((R26-R21)*SQRT(2*R26*R21-R21^2))","v":2.5274078042854149}]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"W = 2*((R^2)-((R-h)^\"))^.5",{"$f":"2*((P28)-(P30))^0.5","v":1.0712142642814275},{"$f":"2*((Q28)-(Q30))^0.5","v":2},{"$f":"2*((R28)-(R30))^0.5","v":1.7320508075688772}]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"100% Full","100% Full","100% Full"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"P26^2*(ACOS((P26-P20)/P26))-((P26-P20)*SQRT(2*P26*P20-P20^2))","v":1.7671458676442586},{"$f":"Q26^2*(ACOS((Q26-Q20)/Q26))-((Q26-Q20)*SQRT(2*Q26*Q20-Q20^2))","v":3.1415926535897931},{"$f":"R26^2*(ACOS((R26-R20)/R26))-((R26-R20)*SQRT(2*R26*R20-R20^2))","v":3.1415926535897931}]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PI*r^2","PI*r^2","PI*r^2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"PI()*(E20/2000)^2","v":1.7671458676442586},{"$f":"PI()*(F20/2000)^2","v":3.1415926535897931},{"$f":"PI()*(G20/2000)^2","v":3.1415926535897931}]
[]
[]
[]
[]
[]
[]
[]
[null,null,"Notes"]
[null,"1)"]
[null,"2)"]
[null,"3)"]
[null,"4)"]
[null,"THIS DOCUMENT IS ISSUED AS PRELIMINARY DESIGN INFORMATION ONLY AND NO LIABILITY IS ACCEPTED OR IMPLIED FOR ACCURACY. ALL DATA SHOULD BE CHECKED AND VERIFIED BY QUALIFIED PERSONNEL. ©KIRK PROCESS SOLUTIONS LIMITED WWW.KIRKPROCESS.COM",null,"Document Title",null,null,null,"Document No."]
[null,null,null,"Level Calculations for",null,null,null,"ABC-12345"]
[null,null,null,"Horizontal  Drum",null,null,null,"Sheet 1 of 1"]